<!DOCTYPE qgis PUBLIC 'http://mrcc.com/qgis.dtd' 'SYSTEM'>
<qgis version="3.34.9-Prizren">
  <identifier></identifier>
  <parentidentifier></parentidentifier>
  <language></language>
  <type>dataset</type>
  <title></title>
  <abstract></abstract>
  <contact>
    <name></name>
    <organization></organization>
    <position></position>
    <voice></voice>
    <fax></fax>
    <email></email>
    <role></role>
  </contact>
  <links/>
  <dates/>
  <fees></fees>
  <encoding></encoding>
  <crs>
    <spatialrefsys nativeFormat="Wkt">
      <wkt>PROJCRS["SIRGAS 2000 / UTM zone 23S",BASEGEOGCRS["SIRGAS 2000",DATUM["Sistema de Referencia Geocentrico para las AmericaS 2000",ELLIPSOID["GRS 1980",6378137,298.257222101,LENGTHUNIT["metre",1]]],PRIMEM["Greenwich",0,ANGLEUNIT["degree",0.0174532925199433]],ID["EPSG",4674]],CONVERSION["UTM zone 23S",METHOD["Transverse Mercator",ID["EPSG",9807]],PARAMETER["Latitude of natural origin",0,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8801]],PARAMETER["Longitude of natural origin",-45,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8802]],PARAMETER["Scale factor at natural origin",0.9996,SCALEUNIT["unity",1],ID["EPSG",8805]],PARAMETER["False easting",500000,LENGTHUNIT["metre",1],ID["EPSG",8806]],PARAMETER["False northing",10000000,LENGTHUNIT["metre",1],ID["EPSG",8807]]],CS[Cartesian,2],AXIS["(E)",east,ORDER[1],LENGTHUNIT["metre",1]],AXIS["(N)",north,ORDER[2],LENGTHUNIT["metre",1]],USAGE[SCOPE["Engineering survey, topographic mapping."],AREA["Brazil - between 48°W and 42°W, northern and southern hemispheres, onshore and offshore."],BBOX[-33.5,-48,5.13,-42]],ID["EPSG",31983]]</wkt>
      <proj4>+proj=utm +zone=23 +south +ellps=GRS80 +towgs84=0,0,0,0,0,0,0 +units=m +no_defs</proj4>
      <srsid>2676</srsid>
      <srid>31983</srid>
      <authid>EPSG:31983</authid>
      <description>SIRGAS 2000 / UTM zone 23S</description>
      <projectionacronym>utm</projectionacronym>
      <ellipsoidacronym>EPSG:7019</ellipsoidacronym>
      <geographicflag>false</geographicflag>
    </spatialrefsys>
  </crs>
  <extent>
    <spatial maxy="0" miny="0" maxz="0" dimensions="2" minx="0" maxx="0" minz="0" crs="EPSG:31983"/>
    <temporal>
      <period>
        <start></start>
        <end></end>
      </period>
    </temporal>
  </extent>
</qgis>
